**BID PREPARED FOR: Casilio Construction**



**PREPARED BY: Ken Casseri**



**2700 Sq. Ft.**

**As pre recommended system by Sherwin Williams**

**300 L.F. Matching Cove**

**1-27-21**

**This proposal outlines the installation process and system recommended to meet the protection and traction necessary for the environmental and chemical conditions at Royal Car Wash.**

**Sherwin Williams Epoxy Broadcast System**

**Country Blue**

**PROCESS**

**Per Manufacturer Spec**

**Grind concrete surface to profile**

**Apply 3579 primer coat**

**Apply wear course coat 3747 with silica broadcast**

**Install matching integral Cove base along all interior walls in wash tunnel.**

**Apply Grout Coat / allow to dry**

**Apply Top Coat 3746**

**Pro Squared is a certified Sherwin Williams Installer**

**(Projected installation time 4 to 5 days)**

**Cost: $15,450**

**NOTE: The coated area should not be exposed to foot or other traffic during the coating processes. Once final top coat is applied, light foot traffic in 24 hours, full cure in 7 days. Payment Schedule**

**50% DUE AT SIGNING / OR 2 WEEKS PRIOR TO START - BALANCE DUE UPON COMPLETION**

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Kenneth A. Casseri Date**

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Customer Signature Date**